NOTE: Use fender covers to avoid damaging painted surfaces.

1. Make sure you have the anti-theft codes for the radio and the navigation system, then write down the frequencies for the radio preset buttons.
   Disconnect the negative (−) cable first, then the positive (+) cable from the battery. Remove the battery.

1. Remove the air cleaner housing.

1. Remove the battery base (A), then remove the ground cable (B).

1. Remove the intake air cover.