1. If necessary, remove the clips and screws, then remove the upper grille molding (A), lower grille molding (B), center grille molding (C), emblem base (D), from the front grille cover (E).

1. Install the front grille in the reverse order of removal, and note these items:
   - Check for damaged or stress-whitened clips, and replace them with new ones.
   - Install the hook portions of the front grille into place securely.