NOTE:

- Do not spill brake fluid on the vehicle; it may damage the paint; if brake fluid does contact the paint, wash it off immediately with water.
- LHD type is shown, RHD type is similar.

1. Remove the brake fluid from the clutch master cylinder reservoir with a syringe.

1. Make sure you have the anti-theft codes for the radio and the navigation system, then write down the frequencies for the radio preset buttons. Disconnect the negative (−) cable first, then the positive (+) cable from the battery. Remove the battery.

1. Remove the air cleaner housing.

1. Remove the battery base.

1. Remove the intake air cover.