Frequent inhalation of brake pad dust, regardless of material composition, could be hazardous to your health.

- Avoid breathing dust particles.
- Never use an air hose or brush to clean brake assemblies. Use an appropriate vacuum cleaner.

1. Raise the rear of the vehicle, and support it with safety stands in the proper location.

1. Remove the rear wheels.

1. Release the parking brake, and remove the rear brake caliper and brake disc/drum.