Center Pillar - Without Side Curtain Airbags SRS components are located in this area. Review the SRS component locations LHD, SRS component locations RHD and the precautions and procedures before performing repairs or service. NOTE:

- Put on gloves to protect your hands.
- Take care not to bend or scratch the trim and panels.
- Use the handy remover set, or equivalent when prying components.

1. Remove these items:
   - Front door sill trim
   - Rear door sill trim
   - Front door opening trim, as needed
   - Rear door opening trim, as needed

1. Remove the center pillar lower trim (A).

   -1. | Detach the lower clips by pulling the bottom of the trim back by hand.
   -2. | Pull the trim down to release the upper hooks (B).

1. Remove the front seat belt upper anchor cover, and remove the upper anchor bolt.