DTC Troubleshooting: 61, 62

DTC 61, 62: High/Low Voltage

1. Clear the DTC using the HDS.

1. Turn the ignition switch ON (II).

Does the ABS indicator come on?

YES | - | Go to Step 3 .
NO | - | The system is OK at this time.■

1. Verify the DTC.

Is DTC 61 or 62 indicated?

YES | - | Check the battery and the charging system. ■
NO | - | Do the appropriate troubleshooting for the DTC indicated.■