LKAS Control Unit DTC 24: Adaptive Cruise Control (ACC) System Malfunction

1. Clear the DTC using the HDS.

1. Turn the ignition switch OFF, then turn it ON (II).

1. Watch the adaptive cruise control (ACC)/LKAS indicator.

Does the adaptive cruise control (ACC)/LKAS indicator come on?

YES | - | Go to Step 4 .
NO | - | Intermittent failure, the system is OK at this time.■

1. Check for LKAS control unit DTCs with HDS.

Is DTC 24 indicated?

YES | - | Troubleshoot the indicated adaptive cruise control (ACC) system DTC(s).■
NO | - | Troubleshoot the indicated DTC.■