NOTE:

- Use the handy remover set, or equivalent when prying components.
- Take care not to tear the seams or damage the seat covers.
- Put on gloves to protect your hands.

1. Remove the seat-back.

1. Remove these items:
   - Armrest (right seat-back)
   - Cargo net (for some models)

1. Remove the lever (A), child seat tether anchor cover (B), and all of the caps (C), then remove all of the screws securing the seat-back top cover (D). The right seat-back is shown; the left seat-back is similar.