Special Tools Required Driver attachment, 78 x 90 mm 07GAD-SD40101 Handle driver 07749-0010000
Driver attachment, 42 x 47 mm
07746-0010300
Snap ring pliers
07LGC-0010100

1. Remove the idler gear shaft when removing the mainshaft bearing and idler gear shaft bearing.
   NOTE: If you are only removing the countershaft bearing, idler gear shaft removal is not needed.

1. To remove the mainshaft bearing (A) and countershaft bearing (B) from the transmission housing, expand each snap ring with the snap ring pliers, then push the bearing out.
   NOTE: Do not remove the snap ring unless it's necessary to clean the grooves in the housing.