NOTE:

- Put on gloves to protect your hands.
- Wear eye protection when removing the glass with piano wire.
- Use seat covers to avoid damaging any surfaces.
- Do not damage the rear window defogger grid lines and terminals.
- Use glass adhesive set P/N 08C73-X0230N.

1. Remove these items:
   - Tailgate lower trim panel
   - Tailgate spoiler trim
   - Rear window wiper motor

1. Remove the molding (A) from the edge of the rear window. If necessary, cut the molding with a utility knife.