1. Remove the splash shield.

1. Loosen the drain plug in the radiator and drain the engine coolant.

1. Drain the transmission fluid:
   - Manual transmission
   - Automatic transmission

1. Drain the engine oil.

1. Disconnect the stabilizer links.

1. Remove the damper fork.

1. Disconnect the suspension lower arm ball joint.

1. Remove the driveshafts. Coat all precision-finished surfaces with clean engine oil. Tie plastic bags over the driveshaft ends.