M/T Reverse Lockout System Symptom Troubleshooting

Troubleshooting is performed after checking DTCs of PGM-FI.

Symptom | Diagnostic procedure | Also check for
--- | --- | ---
It cannot shift to a reverse gear | 1. 2. | Test the reverse lockout solenoid. Reverse lockout circuit troubleshooting. |
It can shift to a reverse gear at 20 km/h (12 mph) or more speed | 1. 2. | Test the reverse lockout solenoid. Reverse lockout circuit troubleshooting. |