Front Individual Map Light Replacement

With Sunroof

1. Carefully pry off the lens (A) with a small screwdriver.

   Front Map Light: | 8 W x 2

1. Remove the two mounting screws.

1. Disconnect connectors (B).

1. Install the light in the reverse order of removal.

Without Sunroof

1. Carefully pry off the lens (A) with a small screwdriver.

   Front Map Light: | 8 W x 2

1. Remove the two mounting screws.

1. Disconnect the 3P connector (B) from the housing (C).

1. Install the light in the reverse order of removal.