1. Install the seat belt in the reverse order of removal, and note these items:
   - Check that the retractor locking mechanism functions as described.
   - Assemble the washers and bushing on the upper and center anchor bolts as shown.
   - Before installing the anchor bolt, make sure there are no twists or kinks in the rear seat belt.

Upper anchor bolt construction
Center anchor bolt construction