RGB Color This screen verifies that the display unit is receiving the video (R, G, B and Composite sync) signals properly. The three primary colors should all be shown without distortion. The combination of all three should produce a central white section. If any of the colors are missing, troubleshoot for the color signal. If the picture has lines in it or scrolls horizontally, or vertically, troubleshoot for a Composite sync problem. |