Immobilizer Control Unit-Receiver Replacement

1. Remove the dashboard lower cover.

1. Remove the steering column covers.

1. Disconnect the 7P connector (A) from the immobilizer control unit-receiver (B).

1. Remove the two screws and the immobilizer control unit-receiver from the ignition key cylinder (C).

1. Install the immobilizer control unit-receiver in the reverse order of removal.

1. After replacement, check the immobilizer system.