NOTE:

- Use the handy remover set, or equivalent when prying components.
- Take care not to scratch the body or rear the seat covers.
- Right rear seat is shown, and left rear seat is similar.

Seat-back/Seat Side Bolster/Slide Linkage/Center Pivot Bracket

1. Tilt the seat-back forward, and tip the seat cushion up.

1. Remove the front cargo floor.

1. Detach the clips and hooks (A) by lifting the seat side bolster (B) up, and remove it.