DTC 68: Brake Pedal Position Switch

1. Check for other DTCs.

Is another DTC indicated?

YES | - | Do the appropriate troubleshooting for the DTC.■
NO | - | Go to Step 2 .

1. Check the brake pedal position switch.

Is the switch OK?

YES | - | Go to Step 3 .
NO | - | Replace the brake pedal position switch. ■

1. Clear the DTC using the HDS.

1. Disconnect the HDS from the 16P DLC.

1. Turn the ignition switch OFF, then turn it ON (II) again.

1. Test-drive the vehicle.

Does the ABS indicator come on, and is DTC 68 indicated?

YES | - | Go to Step 7 .
NO | - | The system is OK at this time.■

1. Troubleshoot the brake pedal position switch circuit.

Is the brake pedal position switch circuit OK?

YES | - | Substitute a known-good ECM, and recheck:■

- If the problem is gone, replace the original ECM.
- If the problem continues, replace the VSA modulator-control unit.

NO | - | Repair the brake pedal position switch circuit.■