Rotor Slip Ring Test

1. Check for continuity between the slip rings (A).
   - If there is continuity, go to Step 15 .
   - If there is no continuity, replace the rotor assembly.

1. Check for continuity between each slip ring and the rotor (B) and the rotor shaft (C).
   - If there is no continuity, replace the rear housing assembly, and go to Step 16 .
   - If there is continuity, replace the rotor assembly.