Brake system indicator does not go off

1. Turn the ignition switch ON (II).

1. Release the parking brake.

Does the brake system indicator go off after several seconds?

YES | - | The system is OK at this time.■
NO | - | Go to Step 3 .

1. Check the brake fluid level.

Is the level OK?

YES | - | Go to Step 4 .
NO | - | Refill the brake fluid, and recheck.■

1. Check the ABS indicator.

Does the ABS indicator stay on?

YES | - | Read the DTC, and do the applicable troubleshooting for the DTC.■
NO | - | Go to Step 5 .

1. Turn the ignition switch OFF.

1. Check the parking brake switch.

Is the parking brake switch OK?

YES | - | Go to Step 7 .
NO | - | Replace the parking brake switch.■

1. Check the brake fluid level switch.

Is the brake fluid level switch OK?

YES | - | Go to Step 8 .
NO | - | Replace the brake fluid level switch .■

1. Remove the gauge control module.

1. Disconnect the gauge control module connector B (30P).

1. Check for continuity between the gauge control module connector B (30P) terminal No. 13 and body ground.

Is there continuity?

YES | - | Repair short to body ground in the wire between the gauge control module and the parking brake switch.■
NO | - | Go to Step 11 .