NOTE:

- Take care not to scratch the rear bumper and body.
- Put on gloves to prevent damage.

1. Remove the rear bumper skirt trim (A) from the rear bumper (B).

   -1. | Remove the bolts (C, D) and clips (E) from the rear bumper.
   -2. | Remove the nuts (F), then remove the rear bumper skirt trim.

1. Install in the reverse order of removal, and note these items:
   - Check the clips for damage or stress-whitening, and if necessary, replace them with new ones.
   - Push the clips and hooks into place securely.