Brake Hose and Line Inspection

1. Inspect the brake hoses for damage, deterioration, leaks, interference, and twisting.

1. Check the brake lines for damage, rusting, and leaks. Also check for bent brake lines.

1. Check for leaks at hose and line joints and connections, and retighten if necessary.

1. Check the master cylinder and ABS or VSA modulator-control unit for damage and leaks.
   NOTE: Replace the brake hose clip whenever the brake hose is serviced.