1. Without sunroof: Remove the headliner.

   -1. | Remove the front door opening trim (A) and rear door opening trim (B) from each roof portion.
   -2. | With the help of an assistant, release the clip (C), detach the fasteners (D) by pulling the rear portion of the headliner (E) down, and lowering the headliner.
   -3. | Remove the cushion tape (F), then remove the roof harness (G) from the headliner.
   -4. | Remove the headliner through the front passenger's door opening.

LHD
RHD