Under-dash Fuse/Relay Box Connector Locations

Under-dash Fuse/Relay Box

Socket | Ref | Terminal | Connects to
--- | --- | --- | ---
A | 6 | 6 | Dashboard wire harness
Accessory power socket relay | 19 | 4 |
A/F sensor relay | 20 | 4 |
B | 12 | 6 | Engine compartment wire harness
C | 11 | 12 | Engine compartment wire harness
D | 13 | 17 | Engine compartment wire harness
E | 8 | 16 | Floor wire harness
F | 9 | 14 | Floor wire harness
G | 14 | 6 | Not used
H | 15 | 14 | Floor wire harness
I | 10 | 5 | Roof wire harness
Ignition coil relay | 23 | 4 |
J | 27 | 21 | Driver's door subharness
K | 26 | 12 | Driver's door subharness
M | 25 | 3 | MICS (MPCS) service check connector
N | 2 | 45 | Dashboard wire harness
P | 17 | 30 | Dashboard wire harness
PGM-FI main relay 1 | 21 | 4 |
PGM-FI main relay 2 | 24 | 4 |
Power window relay | 22 | 4 |
Q | 16 | 14 | Dashboard wire harness
R | 3 | 2 | Dashboard wire harness
S | 5 | 2 | Dashboard wire harness
Starter cut relay | 18 | 4 |
T | 7 | 6 | Optional connector
Turn signal/hazard relay | 4 | 6 |
X | 1 | 39 | Dashboard wire harness