Front Grille Replacement

NOTE:

- When prying components, use the handy remover set or equivalent.
- Take care not to scratch the front bulkhead cover and front grille.

1. Remove the clips (A, B, C), then remove the front grille cover (D).

1. Remove the clips, then remove the front grille (A).Take care not to drop the clips inside the front bumper.

1. Install the front grille in the reverse order of removal, and note these items:
   - Replace any damaged clips.
   - Install the hook portions of the front grille into place securely.