Exploded View Special Tools Required Driver handle 07NAD-SR30101 Cylinder end seal remover attachment 07NAD-SR30200 Pilot collar 07PAF-0010680 Valve seal ring sizing tool 07NAG-SR30900 Ball joint boot clip guide 07974-SA50800 Sleeve seal ring sizing tool 07974-SA50200 Attachment, 32 x 35 mm 07746-0010100 Driver 07749-0010000 Piston seal ring guide 07HAG-SF10100 Piston seal ring sizing tool 07HAG-SF10200 Cylinder end seal slider 07ZAG-S5A0300 Pincers Oetiker 1098 or equivalent, commercially available NOTE: Refer to the Exploded View as needed during this procedure. The illustrations show LHD model, RHD model is symmetrical. Removal Remove the steering gearbox. |