Install the housing clip (A). Press the brake pedal several times to make sure the brakes work, then test-drive the vehicle. NOTE: Engagement of the brake may require a greater pedal stroke immediately after the brake pads have been replaced as a set. Several applications of the brake pedal will restore the normal pedal stroke. After installation, check for leaks at hose and line joints or connections, and retighten if necessary. Install the front wheels. |