Radiator

Item | Measurement | Qualification | Standard or New
--- | --- | --- | ---
Radiator | Coolant capacities (including engine, heater, hoses, and reservoir) Use genuine Honda All Season Antifreeze/Coolant Type 2 | M/T : engine overhaul | 6.9 L (1.82 US gal, 1.51 Imp gal)
M/T : coolant change | 5.0 L (1.32 US gal, 1.10 Imp gal)
A/T : engine overhaul | 6.6 L (1.74 US gal, 1.45 Imp gal)
A/T : coolant change | 4.7 L (1.24 US gal, 1.03 Imp gal)