TMC Status This screen displays a state about the TMC reception. Frequency: Frequency receiving in this time. Field Strength: Display reception sensitivity with 0−15. 0−5: Cannot receive 6: Instability 7−8: Can receive it somehow 9−15: Can receive it clear Error Rate Correction: RDS block error. Uncorrected Block/min: The number of block errors per one minute. Message Counter: The number of messages which I received. Provider Count: The number of providers which I can receive. Box Error Status: An error of a TMC tuner. |