M/T differential carrier

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
M/T differential carrier | Pinion shaft contact area I.D. |  | 18.010−18.028 mm (0.7091−0.7098 in.) | ———
Carrier-to-pinion shaft clearance |  | 0.027−0.057 mm (0.0011−0.0022 in.) | 0.1 mm (0.004 in.)
Driveshaft contact area I.D. |  | 28.025−28.045 mm (1.1033−1.1041 in.) | ———