NOTE: Put on gloves to protect your hands. Wear eye protection when removing the glass with piano wire. Use seat covers to avoid damaging any surfaces. Do not damage the rear window defogger grid lines and terminals. Use glass adhesive set P/N 08C73-X0230N. Remove these items: Tailgate lower trim panel Tailgate spoiler trim Rear window wiper motor Remove the molding (A) from the edge of the rear window. If necessary, cut the molding with a utility knife. |