Exploded View - Clutch Housing 5-speed model: 6-speed model: Exploded View - Transmission Housing 5-speed model: 6-speed model: NOTE: Place the clutch housing on two pieces of wood thick enough to keep the mainshaft from hitting the workbench. 6-speed model is shown, 5-speed model is similar. Remove the detent bolts (A), springs, steel balls, and back-up light switch (B). Remove the transmission hanger (C), 20 mm bolt (D), and 20 mm washer (E). |