Front Individual Map Light Replacement

1. With Sunroof Carefully pry off the lens (A) with a small screwdriver.
   Front Map Light: | 8 W x 2
Remove the two mounting screws. Disconnect connectors (B). Install the light in the reverse order of removal. |

1. Without Sunroof Carefully pry off the lens (A) with a small screwdriver.
   Front Map Light: | 8 W x 2
Remove the two mounting screws. Disconnect the 3P connector (B) from the housing (C). Install the light in the reverse order of removal. |