Brake Fluid Pressure Sensor
The brake fluid pressure sensors are installed in the right and left sides of the brake line 4-way joint. The brake fluid pressure is converted to a signal (voltage value) and is output to the adaptive cruise control (ACC) unit. The adaptive cruise control (ACC) unit is always monitoring the adaptive cruise control (ACC) brake operation and the brake pressure controlled by the signal sent from the brake fluid pressure sensor.