DTC Troubleshooting: 68

DTC 68: Brake Pedal Position Switch Check for other DTCs. Is another DTC indicated?
YES | - | Do the appropriate troubleshooting for the DTC.■
NO | - | Go to Step 2 .
Check the brake pedal position switch. Is the switch OK?
YES | - | Go to Step 3 .
NO | - | Replace the brake pedal position switch. ■
Clear the DTC using the HDS. Disconnect the HDS from the 16P DLC. Turn the ignition switch OFF, then turn it ON (II) again. Test-drive the vehicle. Does the ABS indicator come on, and is DTC 68 indicated?
YES | - | Go to Step 7 .
NO | - | The system is OK at this time.■
Troubleshoot the brake pedal position switch circuit. Is the brake pedal position switch circuit OK?
YES | - | Substitute a known-good ECM , and recheck: If the problem is gone, replace the original ECM.■ If the problem continues, replace the VSA modulator-control unit. ■
NO | - | Repair the brake pedal position switch circuit.■