NOTE: Do not spill brake fluid on the vehicle; it may damage the paint; if brake fluid does contact the paint, wash it off immediately with water. LHD type is shown, RHD type is similar. Remove the brake fluid from the clutch master cylinder reservoir with a syringe. Make sure you have the anti-theft codes for the radio and the navigation system, then write down the frequencies for the radio preset buttons. Disconnect the negative (−) cable first, then the positive (+) cable from the battery. Remove the battery. Remove the air cleaner housing. Remove the battery base. Remove the intake air cover. |