Remove the hub bearing unit (A) and O-ring (B). Install the hub bearing unit in the reverse order of removal, and note these items: Use a new O-ring on reassembly. Tighten all mounting hardware to the specified torque values. Before installing the brake disc, clean the matching surfaces of the hub bearing unit and brake disc. Before installing the wheel, clean the mating surfaces of the brake disc and the inside of the wheel. Check the wheel alignment, and adjust if necessary. |