SRS components are located in this area. Review the SRS component locations and the precautions and procedures before performing repairs or service. NOTE: Put on gloves to protect your hands. Take care not to damage, wrinkle or twist the carpet. Be careful not to damage the dashboard or other interior trim pieces. Disconnect the negative cable from the battery, and wait at least 3 minutes before beginning work. Remove these items. Front seats, both sides Kick panels, both sides Front door sill trim, both sides Center console Driver's dashboard center lower cover Passenger's dashboard center lower cover Parking brake lever Stereo amplifer Remove these items: Rear door sill trim, both side Center pillar lower trim Rear seat cushion, both sides Remove the front seat belt lower anchor bolt, both sides. Push the knob (A) back to release the hook (B) then pull up the accelerator pedal (C). |