Brake system indicator does not go off Turn the ignition switch ON (II). Release the parking brake. Does the brake system indicator go off after several seconds?
YES | - | The system is OK at this time.■
NO | - | Go to Step 3 .
Check the brake fluid level. Is the level OK?
YES | - | Go to Step 4 .
NO | - | Refill the brake fluid, and recheck.■
Check the ABS indicator. Does the ABS indicator stay on?
YES | - | Read the DTC, and do the applicable troubleshooting for the DTC.■
NO | - | Go to Step 5 .
Turn the ignition switch OFF. Check the parking brake switch. Is the parking brake switch OK?
YES | - | Go to Step 7 .
NO | - | Replace the parking brake switch.■
Check the brake fluid level switch. Is the brake fluid level switch OK?
YES | - | Go to Step 8 .
NO | - | Replace the brake fluid level switch .■
Remove the gauge control module. Disconnect the gauge control module connector B (30P). Check for continuity between the gauge control module connector B (30P) terminal No. 13 and body ground. Is there continuity?
YES | - | Repair short to body ground in the wire between the gauge control module and the parking brake switch.■
NO | - | Go to Step 11 .