Immobilizer Control Unit-Receiver Replacement

Remove the dashboard lower cover. Remove the steering column covers. Disconnect the 7P connector (A) from the immobilizer control unit-receiver (B). Remove the two screws and the immobilizer control unit-receiver from the ignition key cylinder (C). Install the immobilizer control unit-receiver in the reverse order of removal. After replacement, check the immobilizer system. |