DTC Troubleshooting: 65

DTC 65: Brake Fluid Level Check the brake fluid level. Is the level correct?
YES | - | Go to Step 2 .
NO | - | Refill the brake fluid, and recheck.■
Check for short in the GRN/RED wire between the gauge control module and the brake fluid level switch. If OK, check the brake fluid level switch. Is the switch OK?
YES | - | Do the troubleshooting for the gauge control module. ■
NO | - | Replace the brake fluid level switch .■