Remove the splash shield. Loosen the drain plug in the radiator and drain the engine coolant. Drain the transmission fluid: Manual transmission Automatic transmission Drain the engine oil. Disconnect the stabilizer links. Remove the damper fork. Disconnect the suspension lower arm ball joint. Remove the driveshafts. Coat all precision-finished surfaces with clean engine oil. Tie plastic bags over the driveshaft ends. |