Exploded View Special Tools Required Hub dis/assembly tool, 42 mm 07GAF-SD40100 Ball joint remover, 28 mm 07MAC-SL00201 or 07MAC-SL00200 Attachment, 72 x 75 mm 07746-0010600 Attachment, 78 x 90 mm 07GAD-SD40101 Driver 07749-0010000 Support base 07965-SD90100 Knuckle/Hub Replacement Raise the front of the vehicle, and support it with safety stands in the proper locations. Remove the wheel nuts, and front wheel. |