Remove the mounting screws and control knobs (A), then remove the printed circuit board (B). Install the audio unit and printed circuit board in the reverse order of removal. Install the audio-HVAC display module and note these items: Make sure the disconnected connectors plugged in properly, and the antenna lead is connected properly. Enter the anti-theft code for the radio, then enter the customer's radio station presets. | 6 CD type: 1 CD type: Navigation type: