Shift lever does not operate smoothly

Probable cause(s)

1. Transmission range switch defective or out of adjustment
2. Shift cable broken or out of adjustment
3. Joint in shift cable and transmission or body worn

Notes

- Check the D indicator, and check for loose connectors. Inspect the transmission range switch for operation.
- Check for a loose shift cable at the shift lever and the transmission control shaft.