Fuse to Components Index - Under-dash Fuse/Relay Box

Under-dash Fuse/Relay Box

Fuse Number | Amps | Wire Color | Component(s) or Circuit(s) Protected
--- | --- | --- | ---
1 | ——— | ——— | Not used
2 | ——— | ——— | Not used
3 | 15 A | RED/WHT | Daytime running lights relay
——— | Multiplex integrated control unit (with daytime running lights)
4 | 20 A | WHT/BLK | Front passenger's recline motor
5 | 20 A | WHT/GRN | Audio amplifier
6 | 10 A | WHT/BLU | Audio unit, Ceiling light, Courtesy lights, Trunk light, Vanity mirror lights
7 | 10 A | WHT/RED | Alarm control siren, Combination light switch control unit, Gauge control module, Immobilizer control unit−receiver, Imoes unit, Navigation display unit, Navigation unit, Ultrasonic sensor
——— | Multiplex integrated control unit
8 | 20 A | ——— | Multiplex integrated control unit (+ BAT door lock)
9 | 20 A | WHT/RED | Cigarette lighter
10 | 7.5 A | WHT | SRS unit
11 | 30 A | GRN | Windshield wiper motor
12 | 7.5 A | RED/YEL | Multiplex integrated control nuit (for rear fog light)
13 | ——— | ——— | Not used
14 | 20 A | WHT/BLU | Driver's power seat slide motor, Driver's power seat front up-down motor
15 | 20 A | RED/BLK | Seat heater
16 | 20 A | WHT/RED | Driver's power seat recline motor, Driver's power seat rear up-down motor
17 | 20 A | WHT/GRN | Front passenger's power seat slide motor
18 | 15 A | BLK/RED | Alternator, ABS or VSA modulator-control unit, ECM, Glow plug control module, Mass air flow sensor
19 | 15 A | BLK/YEL | Immobilizer control unit-receiver, Imoes control unit
20 | 7.5 A | YEL/GRN | Windshield washer motor, Sunroof open relay, Sunroof close relay, Rain sensor
21 | 7.5 A | YEL | Back-up light, Combination switch control unit, Door multiplex control unit, Gauge control module, Relay control module
——— | Multiplex integrated control unit
22 | 10 A | WHT/RED | SRS unit
23 | ——— | ——— | Not used
24 | 20 A | YEL/RED | Left rear power window motor
25 | 20 A | YEL/BLU | Right rear power window motor
26 | 20 A | GRN/BLK | Front passenger's power window motor
27 | 20 A | GRN/WHT | Driver's power window motor
28 | 20 A | GRN | Sunroof motor
29 | 7.5 A | YEL/BLU | Headlight adjuster unit (without HID), Headlight adjuster switch (without HID), Headlight adjuster control unit (with HID)
30 | 7.5 A | BLK/YEL | A/C compressor clutch relay, Blower motor relay, Climate control unit, Condenser fan relay, ECM, Fan control relay, Power mirror actuator, Power mirror defogger, Radiator fan relay, Rear window defogger relay, Recirculation control motor, Seat heater relay, Magnet valve Optional connector
31 | ——— | ——— | Not used
32 | 7.5 A | YEL/RED | Accessory power socket relay, Audio unit, Audio amplifier, Navigation display unit, Navigation unit, Optional connector
33 | ——— | ——— | Not used