NOTE: Do not spill brake fluid on the vehicle; it may damage the paint; if brake fluid gets on the paint, wash it off immediately with water. Be careful not to damage or deform the brake lines during removal and installation. To prevent the brake fluid from flowing, plug and cover the hose ends and joints with a shop towel or equivalent material. Removal Remove the ground cable (A). Remove the torque rod (B). |