DTC P2118: Throttle Actuator Current Range/Performance Problem Disconnect the throttle actuator control module 16P connector. Measure resistance between throttle actuator control module 16P connector terminals No. 1 and No. 8. Is there about 1.0 Ω or less?
YES | - | Go to Step 3 .
NO | - | Substitute a known-good throttle actuator control module, then go to Step 7 and recheck. If DTC P2118 is not indicated, replace the original throttle actuator control module, then go to Step 7 .
Disconnect the throttle body 6P connector. |