Clutch Disc and Pressure Plate Installation Temporarily install the clutch disc onto the splines of the transmission mainshaft. Make sure the clutch disc slides freely on the mainshaft. Install the ring gear holder. Apply a light coat of urea grease UM264 (P/N 41211-PY5-305) to the crankshaft pilot bushing (A). Apply urea grease UM264 (P/N 41211-PY5-305) to the splines (B) of the clutch disc (C), then install the clutch disc using the special tools. |