SRS components are located in this area. Review the SRS component locations LHD, SRS component locations RHD and the precautions and procedures before performing repairs or service. Remove these items: Headliner Sunroof glass Without side curtain airbag: Rear grab handle bracket, both sides Without side curtain airbag: Roof side pad, front and rear both sides With side curtain airbag: Remove the bolts securing both rear grab handle brackets (A), then release them from the body. Do not pull the bracket with the airbag excessively. Take care not to damage the airbag. |